**TW 12**

**1.0 Ton wall sleeve condensing unit**

* Insulated for sound attenuation
* Installed and serviced from indoors
* 208 / 230V single phase
* G90 Galvanized for long rust free life

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Catalogue No. | Capacity(Tons) | Cabinet dimensions (inches) | RefrigerantLine size | Electrical | CompressorType |
| Width | Height | Depth | Liquid | Vapor | Min Amps | MaxBreaker Amps |
| TW12 | 1.0 | 14.25 | 56 | 16 | 3/8” | 5/8” | 8 | 15 | Rotary |

Print Date:10/5/2014

|  |  |
| --- | --- |
| **Project** |  |
| **Address** |  |
| **Date** |  |